|  |  |  |  |
| --- | --- | --- | --- |
| Latest time for node | 9 | Is | 28 |
| Latest time for node | 8 | Is | 20 |
| Latest time for node | 7 | Is | 16 |
| Latest time for node | 6 | Is | 16 |
| Latest time for node | 5 | Is | 15 |
| Latest time for node | 4 | Is | 10 |
| Latest time for node | 3 | Is | 5 |
| Latest time for node | 2 | Is | 8 |
| Latest time for node | 1 | Is | 0 |

1. The backward pass is carried out to calculate the latest dates on which each activity may be started and finished without delaying the end date of the project.